|  |
| --- |
| **Table 9.4.1.12.2.1 Requirements for accepted development - Township zone - Township convenience precinct** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirements for accepted development** | | **E Compliance**   * **Yes** * **No** | **Council confirmation** |
| **General requirements** | | | |
| **Boundary realignment** | |  |  |
| **RAD1** | Lots created by boundary realignment:   1. have a service connection for each lot to the reticulated water supply, sewerage, electricity and telecommunications networks where the networks are available at any location along the frontage of the created lot to a road confirmed by certification from the service provider; 2. contain all existing service connections to water, sewer, electricity, telecommunication and other infrastructure or utility services wholly within the lot they serve confirmed by certification from a licensed surveyor 3. have a minimum 4 metre wide point of vehicular access into the lot from a sealed road having a minimum clearance of 1 metre to any pole, stormwater gully pit, traffic island, item of street furniture, street tree, or the like in the road; 4. do not require additional infrastructure connections or modification to existing connections. 5. do not result in the creation of any additional lots; 6. have easements connected to existing lots extended to the corresponding created lot(s) when not proposed to be extinguished as a result of the boundary realignment |  |  |
| **RAD2** | Boundary realignment does not result in existing land uses on site becoming non-complying with planning scheme requirements   |  | | --- | | Note - Examples may include but are not limited to:   1. minimum lot size requirements; 2. minimum or maximum required setbacks 3. parking and access requirements; 4. servicing and Infrastructure requirements; 5. dependant elements of an existing or approved land use being separately titled. | |  |  |
| **RAD3** | Boundary realignment does not result in the creation of additional building development opportunity within a mapped buffer or separation area; |  |  |
| **RAD4** | No new boundaries are located within 2m of High Value Areas as identified in Overlay map - Environmental areas. |  |  |
| **RAD5** | Boundary realignment does not result in the clearing of any Habitat trees. |  |  |